EXTERNAL FLOW WORK

SET THE EQUIPMENT

TRANSFER TO CAD THE 3D POINT CLOUD AND ANALYSE THE DIMENSIONS

WHEN IT'S DONE, GET THE SD CARD

START THE SCANNER

CHECK POSITION THE CORD GUIDE

INSERT A SD CARD

VERIFY THE WATHER LEVEL ON THE CAISSON